**PhoneTorch A7+**

User Manual

**Introduction**

To make the best use of your PhoneTorch, please read this manual carefully.

Phone setting

1. Phone turn on/off

Please press the on-hook for a 3 second to open turn on/off the phonetorch

Unlock

If the screen is locking, please press the “-” then press the”#” for unlock.

Setting

Language setting, setting—phone setting—language setting—choose your language

SIM Card use

After insert the SIM Card, A7+ will automatic identification, and it is supports

dual SIM dual stanby, you can insrt one micro and one standard SIM card at the same time.

TF Card use

Turn off the phonetorch and move out the battery, then insert the TF Card to the TF Card slot.

Battery charging

1. Input: Open the USB slot cover, put the USB micro port insert the micro usb slot for charging.

Factory Reset

Options for restoration of factory setting, Press the prompt for phone password, press “OK”

Password：1234

volume adjustment

setting—profiles—Options—Adjust volume

or

Direct to Andio player press up and down key

Power Bank use

Open the USB slot cover, find the male USB slot, connect phonetorch and other phone with USB for charging as power bank

Loudspeaker use

Put your favorite music in TF card, then insert A7+ TF card slot. Choose the multimedia for playing

Flashlight use

1. turn the flashlight key on, with key is on the side

FAQ

|  |  |
| --- | --- |
| Question | Solve |
| Can`t not power on | 1. whether press “power on key” for 3second or not 2. Open back case to remove the in sulating tape on battery before startup 3. Whether the battery is running down or not |
| Call quality is poor | 1. Please check the volume 2. Maybe the sign is not good   Change your calling place |
| SIM card error | 1. SIM card is not put right 2. These are pollutant on SIM, please clean it 3. SIM was breakdown |
| Can`t charge for oher phone | 1. check the usb whether is breakdown or not 2. check the usb whether is Compatible with your phone or not 3. the phonetorch`s battery is deplete |